Useful specification

Stable

Long battery life

Easy to control

Auto leveling

Stable flight

Ability to mount a swiveling camera mount

Instructions

1. Place drone on a flat surface
2. Plug battery in
3. Wait for calibration to end
4. Turn on remote
5. With the throttle all the way down move the stick left to start the motors
6. When done to stop the motors move the throttle all the way down then to the right